USB Flash Drive Boot Reference List

*Prepared by Remruata Ralte*

*E-mail – ralteads@gmail.com*

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Manufacturer | Type | Models | Boot Menu | Boot Once | BIOS/UEFI Key | Change Priority |
| Acer |   |   | Esc, F12, F9 |   | Del, F2 |   |
| Acer | netbook | Aspire One zg5, zg8 | F12 |   | F2 |   |
| Acer | netbook | Aspire Timeline | F12 |   | F2 |   |
| Acer | netbook | Aspire v3, v5, v7 | F12 | The "F12 Boot Menu" must be enabled in BIOS. It is disabled by default. | F2 |   |
| Manufacturer | Type | Models | Boot Menu | Boot Once | BIOS/UEFI Key | Change Priority |
| Apple |   | After 2006 | Option |   |   |   |
| Manufacturer | Type | Models | Boot Menu | Boot Once | BIOS/UEFI Key | Change Priority |
| Asus | desktop |   | F8 |   | F9 |   |
| Asus | laptop | VivoBook f200ca, f202e, q200e, s200e, s400ca, s500ca, u38n, v500ca, v550ca, v551, x200ca, x202e, x550ca, z202e | Esc |   | Delete |   |
| Asus | laptop | N550JV, N750JV, N550LF, Rog g750jh, Rog g750jw, Rog g750jx | Esc | Disable "Fast Boot" and "Secure Boot Control" in order to boot from MBR formatted media. | F2 |   |
| Asus | laptop | Zenbook Infinity ux301, Infinity ux301la, Prime ux31a, Prime ux32vd, R509C, Taichi 21, Touch u500vz, Transformer Book TX300 | Esc | Disable "Fast Boot" and "Secure Boot Control" in order to boot from MBR formatted media. | F2 |   |
| Asus | notebook | k25f, k35e, k34u, k35u, k43u, k46cb, k52f, k53e, k55a, k60ij, k70ab, k72f, k73e, k73s, k84l, k93sm, k93sv, k95vb, k501, k601, R503C, x32a, x35u, x54c, x61g, x64c, x64v, x75a, x83v, x83vb, x90, x93sv, x95gl, x101ch, x102ba, x200ca, x202e, x301a, x401a, x401u, x501a, x502c, x750ja | F8 |   | DEL |   |
| Asus | netbook | Eee PC 1015, 1025c | Esc |   | F2 | Boot Tab, Boot Device Priority, 1st Boot Device, Removable Device, F10 |
| Manufacturer | Type | Models | Boot Menu | Boot Once | BIOS/UEFI Key | Change Priority |
| Compaq |   | Presario | Esc, F9 |   | F10 | BIOS "Advanced Tab", Boot Order |
| Manufacturer | Type | Models | Boot Menu | Boot Once | BIOS/UEFI Key | Change Priority |
| Dell | desktop | Dimension, Inspiron, Latitude, Optiplex | F12 | Select "USB Flash Drive". | F2 |   |
| Dell | desktop | Alienware Aurora, Inspiron One 20, Inspiron 23 Touch, Inspiron 620, 630, 650, 660s, Inspiron 3000, X51, XPS 8300, XPS 8500, XPS 8700, XPS 18 Touch, XPS 27 Touch | F12 | Select "USB Flash Drive". | F2 |   |
| Dell | desktop | Inspiron One 2020, 2305, 2320, 2330 All-In-One | F12 | Select "USB Flash Drive". | F2 |   |
| Dell | laptop | Inspiron 11 3000 series touch, 14z Ultrabook, 14 7000 series touch, 15z Ultrabook touch, 15 7000 series touch, 17 7000 series touch | F12 | Select "USB Storage Device" | F2 | Settings->General->Boot Sequence->"USB Storage Device", then up arrow, [Apply]--[Exit] |
| Dell | laptop | Inspiron 14R non-touch, 15 non-touch, 15R non-touch, 17 non-touch, 17R non-touch | F12 | Select "USB Storage Device" | F2 | Settings->General->Boot Sequence->"USB Storage Device", then up arrow, [Apply]--[Exit] |
| Dell | laptop | Latitude c400, c600, c640, d610, d620, d630, d830, e5520, e6320, e6400, e6410, e6420, e6430, e6500, e6520, 6430u Ultrabook, x300 | F12 | Select "USB Storage Device" from boot menu. | F2 |   |
| Dell | laptop | Precision m3800, m4400, m4700, m4800, m6500, m6600, m6700, m6800 | F12 | Select "USB Storage Device" from boot menu. | F2 |   |
| Dell | laptop | Alienware 14, Alienware 17, Alienware 18, XPS 11 2-in-1, XPS 12 2-in-1, XPS 13, XPS 14 Ultrabook, XPS 15 Touch, | F12 | Select "USB Storage Device" from boot menu. | F2 |   |
| Manufacturer | Type | Models | Boot Menu | Boot Once | BIOS/UEFI Key | Change Priority |
| eMachines |   |   | F12 |   | Tab, Del |   |
| Manufacturer | Type | Models | Boot Menu | Boot Once | BIOS/UEFI Key | Change Priority |
| Fujitsu |   |   | F12 |   | F2 |   |
| Manufacturer | Type | Models | Boot Menu | Boot Once | BIOS/UEFI Key | Change Priority |
| HP | generic |   | Esc, F9 |   | Esc, F10, F1 |   |
| HP | desktop | Pavilion Media Center a1477c | Esc |   | F10 | BIOS "Advanced" tab, Boot Order, Move "USB Device" before "Hard Drive" |
| HP | desktop | Pavilion 23 All In One | Esc | Select boot media from the menu. | F10 | UEFI/BIOS "Advanced" tab, Boot Order, Move "USB Device" before "Hard Drive". For non-UEFI media, disable secure boot and enable legacy support. |
| HP | desktop | Pavilion Elite e9000, e9120y, e9150t, e9220y, e9280t | Esc, F9 |   | F10 |   |
| HP | desktop | Pavilion g6 and g7 | Esc |   | F10 | UEFI/BIOS "Advanced" tab, Boot Order, Move "USB Device" before "Hard Drive" |
| HP | desktop | Pavilion HPE PC, h8-1287c | Esc | Then F9 for "Boot Menu" | Esc | F10, Storage tab, Boot Order, Legacy Boot Sources |
| HP | desktop | Pavilion PC, p6 2317c | Esc | Then F9 for "Boot Menu" | Esc | F10, Storage tab, Boot Order, Legacy Boot Sources |
| HP | desktop | Pavilion PC, p7 1297cb | Esc | Then F9 for "Boot Menu" | Esc | F10, Storage tab, Boot Order, Legacy Boot Sources |
| HP | desktop | TouchSmart 520 PC | Esc | Then F9 for "Boot Menu" | Esc | F10, Storage tab, Boot Order, Legacy Boot Sources |
| HP | laptop | 2000 | Esc | Then F9 for "Boot Menu". Select "Patriot Memory" on the Boot Option Menu. | Esc | Then F10, Storage tab, Boot Order, Legacy Boot Sources |
| HP | notebook | Pavilion g4 | Esc |   | F10 | BIOS "Advanced" tab, Boot Order, Move "USB Device" before "Hard Drive" |
| HP | notebook | ENVY x2, m4, m4-1015dx, m4-1115dx, sleekbook m6, m6-1105dx, m6-1205dx, m6-k015dx, m6-k025dx, touchsmart m7 | Esc | Then F9 for "Boot Menu" | Esc | Then F10, Storage tab, Boot Order, Legacy Boot Sources |
|  |  |  |  |  |  |  |
| HP | notebook | Envy, dv6 and dv7 PC, dv9700, Spectre 14, Spectre 13 | Esc | Then F9 for "Boot Menu" | Esc | Then F10, Storage tab, Boot Order, Legacy Boot Sources |
| HP | notebook | 2000 - 2a20nr, 2a53ca, 2b16nr, 2b89wm, 2c29wm, 2d29wm | Esc | Then F9 for "Boot Menu" | Esc | Then F10, Storage tab, Boot Order, Legacy Boot Sources |
| HP | notebook | Probook 4520s, 4525s, 4540s, 4545s, 5220m, 5310m, 5330m, 5660b, 5670b | Esc |   | F10 | BIOS "Advanced" tab, Boot Order, Move "USB Device" before "Hard Drive" |
| HP | tower | Pavilion a410n | Esc |   | F1 | BIOS "Boot" tab, Boot Device Priority, Hard Drive Boot Priority, Move "USB-HDD0" up to #1 position. |
| Manufacturer | Type | Models | Boot Menu | Boot Once | BIOS/UEFI Key | Change Priority |
| Intel |   |   | F10 |   |   |   |
| Manufacturer | Type | Models | Boot Menu | Boot Once | BIOS/UEFI Key | Change Priority |
| Lenovo | desktop |   | F12, F8, F10 |   | F1, F2 |   |
| Lenovo | laptop |   | F12 |   | F1, F2 |   |
| Lenovo | laptop | ThinkPad edge, e431, e531, e545, helix, l440, l540, s431, t440s, t540p, twist, w510, w520, w530, w540, x140, x220, x230, x240, X1 carbon | F12 |   | F1 |   |
| Lenovo | laptop | IdeaPad s300, u110, u310 Touch, u410, u510, y500, y510, yoga 11, yoga 13, z500 | Novobutton | Small button on the side next to the power button. | Novo button | Small button on the side next to the power button. |
| Lenovo | laptop | IdeaPad P500 | F12 or Fn + F11 |   | F2 |   |
| Lenovo | netbook | IdeaPad S10-3 | F12 |   | F2 |   |
| Lenovo | notebook | g460, g470, g475, g480, g485 | F12 |   | F2 |   |
| Manufacturer | Type | Models | Boot Menu | Boot Once | BIOS/UEFI Key | Change Priority |
| NEC |   |   | F5 |   | F2 |   |
| Manufacturer | Type | Models | Boot Menu | Boot Once | BIOS/UEFI Key | Change Priority |
| Packard Bell |   |   | F8 |   | F1, Del |   |
| Manufacturer | Type | Models | Boot Menu | Boot Once | BIOS/UEFI Key | Change Priority |
| Samsung |   |   | F12, Esc |   |   |   |
| Samsung | netbook | NC10 | Esc |   | F2 | Boot Tab, Select "Boot Device Priority", Press Return, Up/Down to Highlight, F6/F5 to change priority. |
| Samsung | notebook | np300e5c, np300e5e, np350v5c, np355v5c, np365e5c, np550p5c | Esc |   | F2 | Boot Tab, Select "Boot Device Priority", Press Return, Up/Down to Highlight, F6/F5 to change priority. |
| Samsung | ultrabook | Series 5 Ultra, Series 7 Chronos, Series 9 Ultrabook | Esc | Note that you must first disable fast boot in BIOS/UEFI to boot from a USB drive. | F2 | Boot Tab, Select "Boot Device Priority", Press Return, Up/Down to Highlight, F6/F5 to change priority. |
| Samsung | ultrabook | Ativ Book 2, 8, 9 | F2 | Note that you must first disable fast boot in BIOS/UEFI to boot from a USB drive or use the F2 boot menu. | F10 | Boot Tab, Select "Boot Device Priority", Press Return, Up/Down to Highlight, F6/F5 to change priority. |
| Manufacturer | Type | Models | Boot Menu | Boot Once | BIOS/UEFI Key | Change Priority |
| Sharp |   |   |   |   | F2 |   |
| Manufacturer | Type | Models | Boot Menu | Boot Once | BIOS/UEFI Key | Change Priority |
| Sony |   | VAIO Duo, Pro, Flip, Tap, Fit | assistbutton |   | assist button |   |
| Sony |   | VAIO, PCG, VGN | F11 |   | F1, F2, F3 |   |
| Sony |   | VGN | Esc, F10 |   | F2 | BIOS "BOOT" section, "External Device Boot" enabled |
| Manufacturer | Type | Models | Boot Menu | Boot Once | BIOS/UEFI Key | Change Priority |
| Toshiba | laptop | Kira, Kirabook 13, Ultrabook | F12 |   | F2 |   |
| Toshiba | laptop | Qosmio g30, g35, g40, g50 | F12 |   | F2 |   |
| Toshiba | laptop | Qosmio x70, x75, x500, x505, x870, x875, x880 | F12 |   | F2 |   |
| Toshiba |   | Protege, Satellite, Tecra | F12 |   | F1, Esc |   |
| Toshiba |   | Equium | F12 |   | F12 |   |